**Helicopter** **transmission gearbox fault detection using an enhanced minimum entropy deconvolution adjusted method**

Xin Zhang1,2, Jiaxu Wang1, Zhiwen Liu1, Jérôme Antoni2

1 School of Aeronautics and Astronautics, Sichuan University, Chengdu, Sichuan 610065, PR China

2 Laboratoire Vibrations Acoustique, Univ Lyon, INSA-Lyon, LVA EA677, F-69621 Villeurbanne, France

Email: zhangx\_15@126.com (Xin Zhang)

**Abstract**

Blind deconvolution (BD) has a very successful application on impulse extracting from amplitude anomalies in vibration recordings for machinery health monitoring and diagnostics. In this paper, we investigate the effect of an exponential transformation on the improvement of the performance of the minimum entropy deconvolution adjusted (MEDA) method for the extracting of periodic fault impulse trains. Meanwhile, based on the exponential transformation, a new varimax norm is defined as criterion for BD. The modified MEDA method is compared to the classical minimum entropy deconvolution (MED), the MEDA, the optimal minimum entropy deconvolution adjusted (OMEDA) on both simulated and experimental signals. The experimental data is from the seeded fault test of H-60 helicopter transmission gearbox. The results show that the modified MEDA performs considerably better than other comparison methods in the extracting of periodic fault impulse trains especially for incipient faults.

**Keywords:** Fault detection; helicopter gearbox; blind deconvolution; minimum entropy deconvolution adjusted; exponential transformation

**References:**

1. Buzzoni, Marco, Jérôme Antoni, and Gianluca D'Elia. "Blind deconvolution based on cyclostationarity maximization and its application to fault identification." Journal of Sound and Vibration 432 (2018): 569-601.
2. Obuchowski, Jakub, Radosław Zimroz, and Agnieszka Wyłomańska. "Blind equalization using combined skewness–kurtosis criterion for gearbox vibration enhancement." Measurement 88 (2016): 34-44.
3. McDonald, Geoff L., Qing Zhao, and Ming J. Zuo. "Maximum correlated Kurtosis deconvolution and application on gear tooth chip fault detection." Mechanical Systems and Signal Processing 33 (2012): 237-255.
4. Ooe, M., and T. J. Ulrych. "Minimum entropy deconvolution with an exponential transformation." Geophysical Prospecting 27.2 (1979): 458-473.
5. Sacchi, Mauricio D., Danilo R. Velis, and Alberto H. Cominguez. "Minimum entropy deconvolution with frequency-domain constraints." Geophysics 59.6 (1994): 938-945.
6. McDonald, Geoff L., and Qing Zhao. "Multipoint optimal minimum entropy deconvolution and convolution fix: Application to vibration fault detection." Mechanical Systems and Signal Processing 82 (2017): 461-477.